// (C) 2006, Michael Gruhn.

// NO WARRANTY IS GRANTED. THIS PLUG-IN IS PROVIDED ON AN "AS IS" BASIS, WITHOUT
// WARRANTY OF ANY KIND. NO LIABILITY IS GRANTED, INCLUDING, BUT NOT LIMITED TO,
// ANY DIRECT OR INDIRECT,  SPECIAL,  INCIDENTAL OR CONSEQUENTIAL DAMAGE ARISING
// OUT OF  THE  USE  OR INABILITY  TO  USE  THIS PLUG-IN,  COMPUTER FAILTURE  OF
// MALFUNCTION INCLUDED.  THE USE OF THE SOURCE CODE,  EITHER  PARTIALLY  OR  IN
// TOTAL, IS ONLY GRANTED,  IF USED IN THE SENSE OF THE AUTHOR'S INTENTION,  AND
// USED WITH ACKNOWLEDGEMENT OF THE AUTHOR. FURTHERMORE IS THIS PLUG-IN A  THIRD
// PARTY CONTRIBUTION,  EVEN IF INCLUDED IN REAPER(TM),  COCKOS INCORPORATED  OR
// ITS AFFILIATES HAVE NOTHING TO DO WITH IT.  LAST BUT NOT LEAST, BY USING THIS
// PLUG-IN YOU RELINQUISH YOUR CLAIM TO SUE IT'S AUTHOR, AS WELL AS THE CLAIM TO
// ENTRUST SOMEBODY ELSE WITH DOING SO.


desc:Amplitude Modulator
//tags: processing amplitude modulation
//author: LOSER

slider1:440<80,1000,1>Frequency (Hz)

in_pin:left input
in_pin:right input
out_pin:left output
out_pin:right output

@slider
x=(2*$pi*slider1)/srate;

@sample
spl0=spl0*sin(t);
spl1=spl1*sin(t);

t=t+x;

